
产品规格书

PRODUCT SPECIFICATION

Customer:

Customer’s part number:

Product description:          433MHz Rubber Antenna       

Uni Link’s part number:       MS-433LSW- 0003
Issue Date:                 2012-12-30

Note:                      433±3 MHz,   SMA  male

Application and Features 

          Applications :  

1： 433MHz ISM band applications
                    2： ISM, RFID applications
                    3： Remote antenna location for better reception
             Features :  

1： 3dBi gain
                    2： Flexible whip
                    3： Indoor use
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1、产品技术指标（SPECIFICATIONS）
	 电性能指标Electrical Specifications

	频率范围Frequency Range (MHz)
	433±3

	频带宽度Bandwidth (MHz)
	6

	输入阻抗Input Impedance (Ω)
	50

	电压驻波比V.S.W.R
	≤ 2.0

	增益Gain (dBi)
	3

	最大输入功率Max Input Power (W)
	5

	机械指标Mechanical Specifications

	天线长度Antenna Length (mm)
	210

	连接器型号Connect Type
	SMA male(用户指定)

	外壳颜色Radome Color
	黑色Black

	重量Weight (g)
	21


2、产品图片（PICTURE）
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3、产品规格图 (DRAWING)
	单位：mm   比例：1:1
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4、机械性能（MECHANICAL CHARACTERISTICS）

	1


	摇摆测试BENDING TEST


	放离接头30CM的线端上荷重120g，固定接头后进行遥摆测试，遥摆角度左右各60度， 遥摆1000次后测试特性.

Put load 120g to 30cm cable from the end of the connector, fixed joints, swaying test at an angle of 60 degrees , test features after 1000 times


	特性无任何现象显示电器性能之损坏.

after 1000 times test no visible damage


	2


	强度测试

STRENG TEST


	一个15磅之静负荷施加放线端底部持续一分钟.
Put 15pounds static load  to the end of the cable continue 1 minute  


	无任何现象显示机械及电器性能之损坏.
After test no visible damage


	3 


	振动测试VIBRATION TEST


	以1.10mm和振幅和33.30Hz/sec振动频率以X轴方向振动120分钟，Y轴方向振动120分钟，Z轴方向振动240分钟.
the X-axis direction for 120 minutes, and the Y-axis direction 120 minutes, the Z-axis direction 240 minutes as vibration testing of 1.1mm amplitude and 33.30Hz/sec of frequency 

	无任何现象显示电器性能之损坏.

After test  no visible damage



5、耐久性测试（DURABILITY）

	1


	盐雾试验

SAIT SPRAY TEST


	盐水喷雾试验：依GB1266-86标准

蒸馏水：一次蒸馏

PH6.5~7

喷雾量：1.4me80cm²/h

压缩空气压力：1Kgf/ cm²

试验相对度：98°

温度：45°~47°

压力温度：35°

测试时间：24hr


	所有规格变华范围初始值30%

 All characteristic range is 30% of the initial value

	2


	高温试验

HEAT TEST
	在85+2℃环境中放24小时，再放在正常环境中30分钟后进行测试

85+2℃ for 24 hours, after keep in normal condition for 30mim the to test.

	

	3


	温试验

HUMIDITY TEST
	在40+2℃ 90-95%RH环境中放24小时，再放在正常环境中30分钟后进行测试 40+2℃ 90-95%RH for 24hours, after keep in normal condition for 30mim the to test.

	

	4


	底温试验

COLD TEST


	在-40+2℃ 环境中放24小时，再置放正常环境中30分钟后进行测试

-40+2℃ for 24hours, after keep in normal condition for 30mim the to test.

	


6、驻波图（VSWR）
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7、辐射图 （RADIATION PATTERN）
[image: image4.png]


[image: image5.png]E-plane Radiation

7120 —stand

—small

~—big gr
~——big gr

(dBi

180





4

